*********************************
*			        *
*     SBB Be6/8 II	 	*
*       Cabview			*
*        MadMike 2001 		*
*    thefarm@t-online.de	*
*      29.09.01 23:00 CET   	*
*                               *
*********************************

Do a normal installation of the Be 6/8.

Put the files from the Zips into the folder /BE68/CAPVIEW 

If you allready have the Be 6/8 installed and the files from the Acela are in 
 /Be68/CAPVIEW delete them and put the files from the zip in there. 

take the folder SOUND  still from the folder ACELA


MadMike

http://www.mikemad.de/msts.htm
